auto lo

iface lo inet loopback
iface eth0 inet dhcp
address 192.168.2.22
netmask 255.255.255.0
gateway 192.168.2.254
dns-nameservers 8.8.8.8, 4.2.2.2

iface wlan0 inet static
address 192.168.50.99
netmask 255.255.255.0
post-up service udhcpd start
